[Common]
CPU usage - Quality (new style)=1
Latency (samples)=4096
Pre amplifier=8
Post amplifier=0.930000007
Extra loudness=1.200000048
Extra loudness - Very deep bass relative clipping level=0
Extra loudness - De-esser limit=130000
Extra loudness - Deep bass protection - Enabled=1
Extra loudness - Deep bass protection - Difference=0
Extra loudness - Deep bass protection - Value=0.638750076
Extra loudness - Forcibly remove DC component caused by Loudness=0
Extra loudness - Reflection strength=0.099999994
Extra loudness - Allow more distortion=0
Extra loudness - Advanced Highs Protection enabled=1
Extra loudness - Advanced Highs Protection - Strength=4
Extra loudness - Advanced Highs Protection - Maximum reduction=1
Extra loudness - New Bass Protection - Clip very deep bass at=0.709999979
Extra loudness - Voice vibrations - Never reduce bass below=0
Extra loudness - Voice vibrations - Allowed graininess multiplication=1
Extra loudness - Non constant sound vibrations - Sensitivity=1
Extra loudness - New Bass Protection - Strict clipping frequency 1=150
Extra loudness - New Bass Protection - Strict clipping frequency 2=250
Extra loudness - New Bass Protection - Strict clipping - Never dynamically raise bass level above=0.939999998
Extra loudness - Dirty Bass=0.790000021
Oversample limiters=1
Extra loudness - Take some shortcuts (CPU)=1
Bass protection - Enabled=1
Bass protection - Two steps=0
Bass protection - Clip level=140
Bass protection - Deep bass boost=0
Bass protection - Raise clip level if highs get above=150
Bass protection - Maximum clip level raise=35
Extra loudness - Clipping strictness=10
Bass protection - Smoothe mid frequencies=4
Bass protection - Smoothe peak detection steepness=0.100000001
Bass protection - Allowed highs distortion=0
Bass protection - Strict bass clipping=1
Extra loudness - Advanced Extreme Highs Protection=1
Extra loudness - Take oversampling shortcuts=1
Hard limit output=0
[Declipper]
Enabled=1
Analog input=0
Maximum restored peak=4
Quality=25
Reduction precision=0.870000005
Maximum expected distortion level=0.110000007
Definitely clipped if below (relative)=0.974999964
Probably clipped if below (relative)=0.774999976
Maybe clipped if below (relative)=0.649999976
Not clipped if below (absolute)=4090
Clipping straight line margin=0.199999988
Clipped if below short term margin=0.199999988
Clipped if below short term margin Enabled=1
Only declip if tilt can be determined=1
Do not allow restored peaks to be lower than clipped signal=0
Do not reconstruct if reconstructed signal resembles original - threshold=1
Do not reconstruct if reconstructed signal resembles original - texture threshold=1
Amount of peak samples to remove - long term=0.100000001
Amount of peak samples to remove - short term=0.400000006
Tilt default level=0
Tilt maximum adjustment per measurement=0.027777778
Tilt level detection enabled=1
Tilt minimum level=-0.125
Tilt maximum level=0.125
Only declip if clipping histogram spike is symmetrical=0
Declip if (type)=3
Declip if type 4 long term margin=0.920000017
Dynamically increase probably clipped level=1
Dynamically increase maybe clipped level=1
Veil normal down speed (dB/ms)=2
Veil after spike down speed (dB/ms)=4
Veil speed drop time reduction time after spike (ms)=1
Veil margin=0.899999976
MP3 margin=0.924999952
MP3 number of samples=1
[FM Hiss]
Enabled=0
Difference=0
FM median pos=25
FM measure max multiplier=2
FM reduce=150
FM delay=2.5
FM delay median=7.502121449
[Noise Gate]
Enabled=1
Difference=0
Noise level=1
Relative noise gate level - Band 1=1
Relative noise gate level - Band 2=1
Relative noise gate level - Band 3=1
Relative noise gate level - Band 4=1
Relative noise gate level - Band 5=1
Relative noise gate level - Band 6=1.247190952
Relative noise gate level - Band 7=1.409638405
[Singleband Compressor]
Enabled=1
Difference=0
Maximum volume=1.169999957
Attack speed=0.004095
Decay speed=0.000539601
Above Top Limiter=1
AGC RMS style Enabled=0
AGC RMS style Target RMS level=25000
AGC RMS style Remove remaining peaks above=1.5
[Pre Compressor]
Enabled=1
Maximum volume - Band 1=33600
Attack speed - Band 1=0.000009075
Attack speed - Band 3=0.000002096
Minimum attack speed near top=0
Force volume down if it is kept too much above calculated target level margin=2
Decay speed - Band 1=0.002375506
Decay speed - Band 3=0.00026822
Dual band=1
Third band=0
Relative expected volume of highs=0.649999976
Relative maximum volume of highs=3
Relative maximum volume of very highs=0.330000013
Remove remaining peaks above (relative to maximum volume)=1.299999952
Remove remaining peaks above (relative to maximum volume) - band 2=1.299999952
Remove remaining peaks in mono=1
Startup input level=0
Maximum expected dynamics strength for smoothing=1
Enable smoothing=0
Smoothing time=0
Gating level=38025
Use ITU-BS.1770 Head=0
Use ITU-BS.1770 Bass=0
Channel separation=0.300000012
Gating based on volume before Pre Amp=0
Lock bass to band 2 strength=0.5
[Pre Compressor Bass]
Enabled=1
Maximum relative volume=1.200000048
Attack speed=0.000050317
Decay speed=0.00214558
Remove remaining peaks above (relative to maximum volume)=1
[Multiband Compressor]
Enabled=1
Difference=0
Delay enabled=0
Maximum volume - Band -1=6270
Maximum volume - Band 0=7290
Maximum volume - Band 1=7290
Maximum volume - Band 2=7120
Maximum volume - Band 3=6440
Maximum volume - Band 4=6780
Maximum volume - Band 5=6610
Maximum volume - Band 6=7120
Maximum volume - Band 7=8810
Maximum volume - Band 8=4580
Attack speeds linked=1
Attack speed - Band -1=0.000282632
Attack speed - Band 0=0.000282632
Attack speed - Band 1=0.000282632
Attack speed - Band 2=0.000282632
Attack speed - Band 3=0.000282632
Attack speed - Band 4=0.000282632
Attack speed - Band 5=0.000282632
Attack speed - Band 6=0.000282632
Attack speed - Band 7=0.000282632
Attack speed - Band 8=0.000282632
Decay speeds linked=1
Decay speed - Band -1=0.000728166
Decay speed - Band 0=0.000728166
Decay speed - Band 1=0.000728166
Decay speed - Band 2=0.000728166
Decay speed - Band 3=0.000728166
Decay speed - Band 4=0.000728166
Decay speed - Band 5=0.000728166
Decay speed - Band 6=0.000728166
Decay speed - Band 7=0.000728166
Decay speed - Band 8=0.000728166
Above Top Limiter=0.75
Clipping enabled=1
Postprocessing enabled=1
Flat frequency response enabled=1
Relative clip position - Band -1=3
Relative clip position - Band 0=1.127659559
Relative clip position - Band 1=1.985074759
Relative clip position - Band 2=1.985074759
Relative clip position - Band 3=1.127659559
Relative clip position - Band 4=1.985074759
Relative clip position - Band 5=1.985074759
Relative clip position - Band 6=1.985074759
Relative clip position - Band 7=1.985074759
Relative clip position - Band 8=0.5625
Final limiter value=1
Final limiter decay speed=0.000700178
Final limiter clipping=1.985074759
Channel separation steepness protection enabled=1
Channel separation steepness (maximum artifact strength)=0.300000012
Equalizer enabled=1
Equalize before multiband-compression=1
Equalizer position - Band -1=1.409638405
Equalizer position - Band 0=1.409638405
Equalizer position - Band 1=1.127659559
Equalizer position - Band 2=1.409638405
Equalizer position - Band 3=1.127659559
Equalizer position - Band 4=2.278688431
Equalizer position - Band 5=1.56410265
Equalizer position - Band 6=1.777777672
Equalizer position - Band 7=1.56410265
Equalizer position - Band 8=0.639344215
Center frequency - Band -1=43.06640625
Center frequency - Band 0=86.1328125
Center frequency - Band 1=172.265625
Center frequency - Band 2=344.53125
Center frequency - Band 3=689.0625
Center frequency - Band 4=1378.125
Center frequency - Band 5=2756.25
Center frequency - Band 6=5512.5
Center frequency - Band 7=10000
Center frequency - Band 8=15000
[Stereo]
Enabled=3
Stereo AZIMUTH Enabled=1
Stereo Image Enabled=1
Stereo Boost Enabled=1
Stereo Boost Excessive Reverb Protection Enabled=0
Delay enabled=0
Difference=0
Center bass=0
AZIMUTH limit=56
AZIMUTH change speed=0.289999992
Image phase amplifier=1
Image phase amplifier maximum angle=180
Image phase amplifier maximum separation strength=100
Image width amplifier=1
Extra phase shift=0
Mono or stereo only=0
Stereo Boost strength=3
Stereo Boost maximum amplification=2.5
Stereo Boost multiplier=1
Stereo Boost - Never reduce below original level=1
[Channel Delay]
Enabled=0
Left Delay=0
[Output Filter]
Enabled=0
Lowpass filter=15000
Highpass filter=20
Highpass filter linearity=Auto
Non-phase-linear highpass filter order=6
Highpass post filter=1
Highpass post filter - avoid artifacts=1
[Bass Boost]
Enabled=1
Strength=1
Start lowpass frequency of input filter=0
End lowpass frequency of input filter=400
Start lowpass frequency of output filter=400
End lowpass frequency of output filter=500
Clip level=1.07889998
Clip level is relative to estimated maximum level=1
Preserve louder peaks=1
Difference=0
[Phase Rotator]
Enabled=0
Start frequency=1070
Start speed=1730
Number of rotations=2.329999924
Smoothness=0.979999959
Low latency look back samples=112
Low latency look ahead samples=20
[Final Limiter]
Enabled=1
Difference=0
Pre-amp=0.840000033
Pre-limiter enabled=0
Pre-limiter relative volume=1.75
Reduced CPU processing=0
[FM Transmitter]
Enabled=0
Pre-emphasize=0
Pre-emphasis time=50
Output is pre-emphasized=0
Stereo encoder enabled=0
RDS encoder enabled=0
Pilot signal volume=9
RDS signal volume=4.5
FM overdrive volume=1
RDS PS text=2s:STEREO/2s:TOOL/<1=1.5s,2..-2=2t,-1=1.5s:WWW.STEREOTOOL.COM/|\W"PLAYING %artist% - %title%        "/1s:\T2h\:\T02m\:\T02s/1s:\T2h\:\T02m\.\T02s/1s:\T2h\:\T02m\:\T02s
RDS RadioText text=60s:Stereo Tool: Professional Audio Processing - www.stereotool.com/30s:Stereo Tool by Hans van Zutphen, 1999-2008 - www.stereotool.com
RDS PTY=0
RDS PI=65535
RDS Alternative frequency 1=0
RDS Alternative frequency 2=0
RDS Alternative frequency 3=0
RDS Alternative frequency 4=0
RDS Alternative frequency 5=0
RDS Alternative frequency 6=0
RDS Alternative frequency 7=0
RDS Alternative frequency 8=0
RDS Alternative frequency 9=0
RDS Alternative frequency 10=0
RDS Alternative frequency 11=0
RDS Alternative frequency 12=0
RDS Alternative frequency 13=0
RDS Alternative frequency 14=0
RDS Alternative frequency 15=0
RDS Alternative frequency 16=0
RDS Alternative frequency 17=0
RDS Alternative frequency 18=0
RDS Alternative frequency 19=0
RDS Alternative frequency 20=0
RDS Alternative frequency 21=0
RDS Alternative frequency 22=0
RDS Alternative frequency 23=0
RDS Alternative frequency 24=0
RDS Alternative frequency 25=0
RDS TP=0
RDS TA=0
RDS Music=1
RDS Artificial Head=0
RDS Compressed=1
RDS Dynamic PTY=0
RDS RadioText Enabled=1
RDS ClockTime Enabled=1
FM Transmitter Calibration Enabled=0
MPX Oversampling mode=Follow main Quality setting
FM Transmitter Calibration - Volume 20 Hz=1
FM Transmitter Calibration - Volume 40 Hz=1
FM Transmitter Calibration - Volume 80 Hz=1
FM Transmitter Calibration - Volume 160 Hz=1
FM Transmitter Calibration - Volume 320 Hz=1
FM Transmitter Calibration - Volume 640 Hz=1
FM Transmitter Calibration - Volume 1280 Hz=1
FM Transmitter Calibration - Volume 2560 Hz=1
FM Transmitter Calibration - Volume 5120 Hz=1
FM Transmitter Calibration - Volume 10240 Hz=1
FM Transmitter Calibration - Volume 19000 Hz=1
FM Transmitter Calibration - Volume 23000 Hz=1
FM Transmitter Calibration - Volume 28000 Hz=1
FM Transmitter Calibration - Volume 33000 Hz=1
FM Transmitter Calibration - Volume 38000 Hz=1
FM Transmitter Calibration - Volume 43000 Hz=1
FM Transmitter Calibration - Volume 48000 Hz=1
FM Transmitter Calibration - Volume 53000 Hz=1
FM Transmitter Calibration - Volume 57000 Hz=1
FM Transmitter Calibration - Phase shift 20 Hz=0
FM Transmitter Calibration - Phase shift 40 Hz=0
FM Transmitter Calibration - Phase shift 80 Hz=0
FM Transmitter Calibration - Phase shift 160 Hz=0
FM Transmitter Calibration - Phase shift 320 Hz=0
FM Transmitter Calibration - Phase shift 640 Hz=0
FM Transmitter Calibration - Phase shift 1280 Hz=0
FM Transmitter Calibration - Phase shift 2560 Hz=0
FM Transmitter Calibration - Phase shift 5120 Hz=0
FM Transmitter Calibration - Phase shift 10240 Hz=0
FM Transmitter Calibration - Phase shift 19000 Hz=0
FM Transmitter Calibration - Phase shift 23000 Hz=0
FM Transmitter Calibration - Phase shift 28000 Hz=0
FM Transmitter Calibration - Phase shift 33000 Hz=0
FM Transmitter Calibration - Phase shift 38000 Hz=0
FM Transmitter Calibration - Phase shift 43000 Hz=0
FM Transmitter Calibration - Phase shift 48000 Hz=0
FM Transmitter Calibration - Phase shift 53000 Hz=0
FM Transmitter Calibration - Phase shift 57000 Hz=0
[Lossy compression output optimization]
Enabled=1
Spike Protation pre-emphasis time=15
[Side Channels]
Channel 1 Enabled=0
Channel 2 Enabled=0
Channel 1 Volume=0
Channel 2 Volume=0
Lowpass frequency=0
[Direct soundcard access]
Enabled=0
Device ID=Realtek Digital Output (Realtek
Volume=1
Buffer size=1
Send to Winamp=Nothing
ASIO Override channel 1=4
ASIO Override channel 2=5
[Low latency output]
Enabled=0
Device ID=ERROR: INVALID DEVICEID
Volume=1
Buffer size=0.080000006
ASIO Override channel 1=2
ASIO Override channel 2=3
